Anti-rising damp cable

The product is supplied entirely wired with anti-rising damp cable. Cable available in two sizes: 2,5 m and 7,5 m.
The neoprene anti-rising damp cable is a type of electrical cable designed with copper strands soaked in a hydrophobic filler that prevents water from rising up inside its sheath, thus ensuring greater safety and durability, especially in wet environments. The neoprene outer jacket offers additional resistance to water, oils, UV rays and adverse weather conditions.

Add 1 or 2to the product code including optics and led colour.
For example LL126100SN (with optic S 25° and led colour N 4000K) if you want to buy it with 7,5 m cable, the
code would become LL126100SN2.

