Ago Q Garden Power



Optic D not available for Honeycomb version. Moisture-resistant cable, AC-Direct version: 0.8 m H05RN-F 3x1. Moisture-resistant cable, 24 V version: 0.8 m H05RN-F 2x0.75.

For the purchase of the product with a longer cable, we recommend the <strong>Standard cable </strong>or the <strong>Anti-rising damp cable.</strong>