Airy Plus Top Ovale 300

Suitable for indoor and outdoor use.
Reflector made of polycarbonate or aluminium type L2-1060.
Silicone gasket.
A4 stainless steel screws.
Cable entry option on the side with rigid tube 16/20 mm.

Lamp max. dim: E27 152 mm Ø 48 mm

Polycarbonate base and diffuser, technopolymer eyelid.
Lamp max. dim: E27 152 mm Ø 48 mm