Beta 4



On-off version cable: 0,7m H05RN-F.
Cable DALI version: 0,7m H07RN-F.
IK 08 5J xx7 with grid accessory.

Also suitable for outdoor use and suspension. Installable on armored cabinet through appropriate bracket, or suspended or ceiling mounted with ceiling bracket. Designed to meet the most complex needs of professional lighting both indoor and outdoor. Wide choice of color temperatures, optics and finishes. Body in die-cast aluminum with finish. Diffuser in transparent glass. Silicone gaskets to maintain IP66 rating, ensuring total protection against dust and powerful water jets from any direction. Stainless steel A4 hardware. The product body is composed of die-cast aluminum; high oxidation resistance thanks to zirconium-based passivation treatment and painting with UV-stabilized polyester resins. Pre-wired fixture with multi-year warranty on LED circuit. <strong>LED 5700K (5), 4000K (N) or 3000K (3). No photobiological risk; RG1 exempt risk group (EN62471).</strong>