CNC 50 2.0 Top 2L

Minimalist downlight for recessed installation. Also suitable for outdoor use. Aluminium body and AISI 316L stainless steel ring nut. Wide choice of colour temperatures. Transparent glass diffuser. The product has an IP 67 rating and is fitted with an integrated Aquastop to protect against water and humidity infiltration. Pre-wired luminaire with multi-year warranty on LED circuit, supplied with power cord H05RN-F 2x0.75. Power supply excluded 24Vdc or 500mA - 6V. 
<strong>LED 4000K (N) or 3000K (3), 2700K (2) or 2200K (1). No photobiological risk under normal conditions of use; RG1 risk group exempt (EN62471).</strong>

Version with Top retaining ring with two 110° openings.