CNC 99 C2L



Bidirectional version.
When installed with recess box code LB1230001, all models are walk-over.
Cod. LL137010N/3/2 stainless steel retaining ring.
The polished stainless steel version is made of AISI 304.