Glow 100 Mask

Also suitable for outdoor use. Integrated 220–240 V driver and latest-generation LED modules. Polycarbonate base, produced using our own injection moulding process. Thick PMMA diffuser. Aluminium cover. Silicone gaskets to maintain IP66 rating. Snap-fit opening and closing mechanism with no screws. Pre-drilled for security screws. Fixing kit included to maintain IP rating. <strong>LEDs: 4000K (N), 3000K (3) or 2700K (2). Direct 220–240V power supply. No photobiological risk under normal conditions of use; RG1 risk group exempt (EN 62471).</strong>

