Kai 2 D4i



D4i-ready. Cable D4i: 0,7m H05RN-F. Recommended for installation on Ø 60 metal poles. Not suitable for Still poles. Model equipped with Zhaga Receptacle at the top of the luminaire and provided with D4i driver.