Punto Stelo

Garden bollard with aluminium pole, ideal for lighting outdoor residential areas. Ground installation using Fischer concrete anchors (supplied). Wide choice of colour temperatures and finishes. Fixed installation. IP 65. Supplied with ‘Seaside’ treatment, ideal for installations in places at greater risk of corrosion. Supplied with a total of 3m of H05RN-F 2x1 cable (cable length from the top of the product). E14 opal lamp power supply. Glossy white glass diffuser. Height 120 cm. The body of the product is made of die-cast aluminium; high resistance to oxidation thanks to zirconium-based passivation treatment and UV-stabilised polyester resin coating. The support bases are supplied in painted steel. A4 stainless steel bolts. <strong>E14 LED lamp supplied in 4000K (N), 3000K (3) or 2700K (2) included. No photobiological risk under normal conditions of use; RG0 risk group exempt (EN62471).</strong>

<strong>PLASTIC SPHERE:</strong> Add “P” to the end of the selected code, including the LED colour, to have the product supplied with a opaque white opal IK07 plastic sphere.
Dimmable bulb, maximum dimensions 80 mm, Ø45 mm.