Punto Tige 500

Ceiling lamp with rigid aluminium rod. Available in lengths of 50 cm and 80 cm. Technopolymer base, aluminium body. Also suitable for outdoor use with IP 65 protection. Glossy white glass diffuser. E14 opal lamp power supply. Wide choice of colour temperatures and finishes. High resistance to oxidation thanks to zirconium-based passivation treatment and UV-stabilised polyester resin coating. Supplied with ‘Bordo Mare’ treatment, ideal for installations in locations at greater risk of corrosion. A4 stainless steel bolts. <strong>E14 LED lamp supplied in 4000K (N), 3000K (3), 2700K (2) included. No photobiological risk under normal conditions of use; RG0 risk group exempt (EN62471).</strong>

<strong>PLASTIC SPHERE:</strong> Add “P” to the end of the selected code, including the LED colour, to have the product supplied with a opaque white opal IK07 plastic sphere.
Dimmable bulb, maximum dimensions 80 mm, Ø45 mm.