Stile Next 106E

Suitable for installation on plasterboard walls and ceilings and for outdoor use.
Body made of EN-AB44100 die-cast aluminium primary alloy; highly resistant to oxidization due to the zirconium-based passivation treatment and UV stabilized polyester resin coating.
Heat tempered and serigraphed glass diffuser.
Silicone gaskets.
A4 or AISI 316L stainless steel nuts and bolts.
Patented model.
<strong>LED 4000K (N) or 3000K (3) LED. Integral ballast 220-240V. 
No risk of photobiological damage, RG0 group (EN62471).</strong>

Double cable entry at the back.
LL653DN/3 ballast not included.