Stile Next 260

Suitable for indoor and outdoor use.
Polycarbonate base and tempered serigraphed glass diffuser.
Reflector made of aluminium type L2-1060.
Silicone gaskets.
PG 13 double cable gland + cover for single power supply.
A4 stainless steel captive hex screws size 2.5 mm.
Patented model.
<strong>LED 4000K (N) or 3000K (3) LED. Integral ballast 220-240V. 
No risk of photobiological damage, RG0 group (EN62471).</strong>
Lamp dim. max: E27 145 mm Ø 48 mm

Lamp dim. max: E27 145 mm Ø 48 mm.