Stile Next 503

Suitable for indoor and outdoor use.
Body made of EN-AB44100 die-cast aluminium primary alloy; highly resistant to oxidization due to the zirconium-based passivation treatment and UV stabilized polyester resin coating.
Heat tempered and serigraphed glass diffuser.
Silicone gaskets.
A4 or AISI 316 L stainless steel nuts and bolts. 
Patented model.
<strong>LED 4000K (N) or 3000K (3). Integral ballast 220-240V. 
No risk of photobiological damage, RG0 group (EN62471).</strong>
Touch screen version available. Only for indoor use.

Single cable entry at the back. 6W version, code LL641D_, not available in 2700K.