Standard cable Ago Garden, Ago Wall, Ago Garden Power, Ago Wall Power

Cable suitable for Ago Garden, Ago Wall, Ago Garden Power, Ago Wall Power.
The product is supplied fully wired with standard cable (H05RN-F 3X1 for AC-DIRECT version, H05RN-F 2X0.75 for 24V version).
Cable available in four sizes: 5 m, 10 m, 15 m and 20 m.
Product supplied with coaxial terminal block 3-pole IP68 terminal block (code LB11293).

Add 4 or 5 or 6 or 7 to the product code including optics and led colour.
For example, LL126100SN (with 25° S-optics and 4000K N-colour LED) if you want to buy it with the addition of the 10 m cable, the code will become LL126100SN5.

