Punto Hasta R Garden

Garden floor lamp with telescopic pole, ideal for lighting residential areas such as outdoor benches and tables. Also suitable for outdoor use with IP65 protection and ground installation. Wide choice of colour temperatures and finishes. Mobile or fixed installation. Also supplied with plug and ‘Bordo Mare’ treatment, ideal for installations in places with a higher risk of corrosion. Supplied with a total of 5m of H05RN-F 2x1 cable (cable length from the top of the product). The product is available in two configurations: Punto Hasta, the standard version with a linear profile, and Punto Hasta R with a calendered profile. E14 opal lamp power supply. Glossy white glass diffuser. Height adjustable from approximately 1.20m to 3m for maximum installation versatility. The body of the product is made of die-cast aluminium; high resistance to oxidation thanks to zirconium-based passivation treatment and UV-stabilised polyester resin coating. The support bases are supplied in painted steel. A4 stainless steel bolts. <strong>E14 LED lamp supplied in 4000K (N), 3000K (3) or 2700K (2) included. No photobiological risk under normal conditions of use; RG0 risk group exempt (EN62471).</strong>

<strong>PLASTIC SPHERE:</strong> Add “P” to the end of the selected code, including the LED colour, to have the product supplied with a opaque white opal IK07 plastic sphere.
Dimmable bulb, maximum dimensions 80 mm, Ø45 mm.